oid setup()

{

// Set pin 8 t/m 10 as output

pinMode(8, OUTPUT);

pinMode(9, OUTPUT);

pinMode(10, OUTPUT);

// Set all output to LOW in order to turn all LEDs off

digitalWrite(8, LOW);

digitalWrite(9, LOW);

digitalWrite(10, LOW);

}

void loop()

{

// Red

digitalWrite(8, HIGH);

delay(5000);

digitalWrite(8, LOW);

// Green

digitalWrite(10, HIGH);

delay(5000);

digitalWrite(10, LOW);

// Orange / Yellow

digitalWrite(9, HIGH);

delay(1000);

digitalWrite(9, LOW);

}